**QUICK SPILL INFORMATION**

**To minimize spill/release impacts, protect storm water drainage inlets!**

* Dam up closest downstream inlet with spill pads and socks and if possible the next downstream inlet
* If the spill/release is a major emergency or high hazard spill/release, call 911
* Call Work Control Center (814-865-4731) to request assistance from the Wastewater Treatment Plant personnel.
	+ Provide location of inlet affected (i.e., west side of facility near intersection of …) and drainage basin (e.g., Main Campus [Duck Pond], Bathgate, Fox Hollow, West Campus, …)
* Call Environmental Health and Safety (814-865-6391)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Small Oil or Chemical Spill, No Storm Water Flow |  | Small Oil Spill, Storm Water Flow |  | Small Chemical Spill, Storm Water Flow |  | Large Chemical or Oil Spill |
|  |
| Absorbents in drain inlet |  | Oil-only absorbent in drain inlet |  | Absorbents in drain inlet |  | Block drain inlets if possible |
|  |  |  |  |  |
| Absorbents in next downstream drain inlet |  | Oil-only absorbent in next downstream inlet | Absorbents in next downstream inlet | Call 911 |
|  |  |  |  |  |  |  |
| Call Work Control Center to initiate WWTP storm drain actions |  | Call Work Control Center to initiate WWTP storm drain actions |  | Call Work Control Center to initiate WWTP storm drain actions |  | Call Work Control Center to initiate WWTP storm drain actions |
|  |  |  |  |  |  |  |
| Call EHS |  | Call EHS |  | Call EHS |  | Call EHS |